SP02820 (2018 Specifications: 10-01-19)

# SECTION 02820 - METAL GUARDRAIL

(Follow all instructions. If there are no instructions above a subsection, paragraph, sentence, or bullet, then include them in the project. The specifications may be modified to include project specific specifications, but all additions, deletions, or modifications must be sent to the ODOT Technical Resource and State Specifications Engineer for review and approval.)

Comply with Section 02820 of the Standard Specifications modified as follows:

**02820.40  Guardrail Anchor Hardware** -  Replace the paragraph that begins “Provide cable and fittings…” with the following paragraph:

Provide cable and fittings for guardrail anchors that conform to the requirements of AASHTO M 30, Class A, for Type II cable. Galvanize all fittings according to AASHTO M 111 (ASTM A123).

**02820.50  Acceptance of Materials** -  Replace this subsection, except for the subsection number and title, with the following:

Acceptance of metal guardrail Materials will be according to Section 00165.35.