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2026 Industrial Stormwater Discharge Permit 
Stormwater Pollution Control Plan Checklist 
Site name:
Permit number:

	Permit Section
	Permit Schedule
	Permit Requirement
	Page #
	Comments
(For official use only)

	New discharger
	Condition
I.1.a or b
	Must satisfy conditions for a new discharger to an impaired water without a TMDL for pH, copper, lead, zinc, iron, E. coli, fecal coliform and enterococcus
	
	

	Signature
	A.15.b
	Signed and certified in accordance with 40 CFR 122.22
	
	

	Title page
	A.15.a
A.17.a
	· Plan date
· Name of:
· Site
· Operator/owner
· Qualified person who prepared the SWCP
· Site contact person (telephone and email)
· Permit number and EPA number (if known)
· SIC codes: primary and co-located
· Physical address, county and mailing address (if different)
· Schedule operating hours
	
	

	Revision log
	A.17.b
	A log for past revision sections and dates
	
	

	General location and site maps
	A.17.d
	Title, legend or key, a north arrow, date and scale
	
	

	General location map
	A.17.d.i (1)
	General location of the site in relation to surrounding properties, transportation routes, surface waters and other relevant features
	
	

	Site map – conveyance
	A.17.d.i
(2)(3)
	Conveyance and discharge structures (pipes, ditches), drainage patterns and flow arrows
	
	

	Site map – monitoring and discharge points
	A.17.d.i (4) A.17.x
	Exact location of all monitoring points labelled with a unique three-digit identifying number starting with 001, 002, etc., labeled “monitoring point” and locations of discharge points if different from monitoring points
	
	

	
Site map – drainage area
	A.17.d.i (5)
(7)
	Outline of the drainage area for each discharge point; locations of discharge points if different from monitoring points
	
	

	Site map – impervious areas
	A.17.d.i
(6)(11)
	Paved areas and buildings within each drainage area; structural features that reduce or minimize impervious areas
	
	

	
Site map – significant materials
	A.17.d.i
(8)(9)
	Areas used for outdoor manufacturing, treatment, storage, or disposal of significant materials and areas of known or discovered significant materials from previous operations
	
	

	Site map – structural controls
	A.17.d.i (10)
	Existing structural control measures for minimizing pollutants in stormwater runoff
	
	

	Site map – material handling
	A.17.d.i
(12)(13)
	Material handling and access areas and hazardous waste treatment, storage and disposal facilities
	
	

	
Site map – water features
	A.17.d.i (14)(15)(16)
	Location of wells including waste injection wells seepage pits, drywells, groundwater wells; springs, wetlands, and other surface waterbodies both on-site and adjacent to the site
	
	

	Site map – authorized non-stormwater
	A.17.d.i (17)
	Location and description of authorized non-stormwater discharges
	
	

	Site map – spill prevention
	A.17.d.i (18)
	Location and description of spill prevention and cleanup materials
	
	

	Site map – 
Locations of the following materials and activities if they are exposed to stormwater and applicable
	A.17.d.i
(19) A-J
	· fueling stations;
· vehicle and equipment maintenance cleaning areas;
· loading/unloading areas;
· locations used for the treatment, storage, or disposal of waste;
· liquid storage tanks;
· processing and storage areas;
· immediate access roads and rail lines used or traveled by carriers of raw materials, manufactured products, waste materials, or by-products used or created by the facility;
· transfer areas for substances in bulk;
· machinery; 
· locations and sources of run-on to your site from adjacent property.
	
	

	Site map – authorized non-stormwater
	A.17.d.i (17)
	Location and description of authorized non-stormwater discharges
	
	

	Site description – industrial activities
	A.17.d.ii
	A description of industrial activities conducted at the site and significant materials stored, used, treated or disposed of in a manner which exposes those activities or materials to stormwater. Include in the description the methods of storage, usage, treatment or disposal
	
	

	Site description – past contamination
	A.17.d.iii
	Location and description, with any available characterization data, of areas of known or discovered significant materials from previous operations
	
	

	Site description – contributing pollutants
	A.17.d.iv
	For each area of the site where a reasonable potential exists for contributing pollutants to stormwater runoff, a description of the potential pollutant sources that could be present in stormwater discharges and if the source is associated with a co-located SIC code
	
	

	Site description – impervious area
	A.17.d.viii
	An estimate of the amount of impervious surface area (including paved areas and building roofs) and the total area drained
by each stormwater discharge point to be reported in area units
	
	

	Site controls – TBELs and WQBELs
	A.17.d.v &
A.8.a-g &
A.20.h.i
	A description of control measures installed and implemented to meet the technology and water quality-based requirements… and any applicable sector-specific requirements in Schedule E;
· Minimize Exposure
· Oil and Grease
· Waste Chemicals and Material Disposal
· Erosion and Sediment Control
· Debris Control
· Dust Generation and Vehicle Tracking
· Housekeeping 
· Water Quality-based Effluent Limits
	
	

	Site controls – source control measures
	A.17.d.v
	Description of how the stormwater control measures address potential pollutant sources from industrial activities and significant materials on-site, spills and leaks and authorized non-stormwater discharges
	
	

	Site controls – treatment
	A.17.d.vi
	Description of stormwater treatment controls or source controls, including low impact development, and implementation dates of approved Tier 2 corrective action response, including approved background waiver
	
	

	Receiving waters
	A.17.d.ix
	The name(s) of the receiving water(s), latitude and longitude of discharge points, and applicable SIC code, if facility has co-located operations
	
	

	Receiving waters – MS4
	A.17.d.ix
	If discharge point is to a municipal storm sewer system, name(s) and latitude and longitude of the receiving water and municipality
	
	

	Housekeeping schedule
	A.17.d.v
	Include known maintenance schedules and frequency of housekeeping measures
	
	

	Preventative maintenance schedule – spills and leaks
	A.8.i
A.17.f
	Procedures for inspecting and cleaning, maintaining and repairing all industrial equipment and systems and materials handling and storage areas that are exposed to stormwater to avoid situations that may result in leaks, spills, and other potential releases of pollutants from drums and tanks
	
	

	Preventative maintenance schedule – BMPs and treatment
	A.8.i
A.17.f
	Schedules or frequency of cleaning, maintaining and repairing all control measures, including stormwater structures and temporary measures, catch basins, and treatment facilities to ensure effective operation as designed
	
	

	Preventative maintenance schedule – treatment
	A.17.g
	Monitoring or inspection plan and frequency and for passive treatment routine maintenance standards
	
	

	Waste collection schedule
	A.17.f
	Schedules of waste collection
	
	

	Spill prevention and response – 
Spills Prevention, Control, and Countermeasure required by other regulations may be substituted for this provision if the spill prevention plan addresses stormwater management
concerns and the plan is included with the SWPCP
	A.17.e.i
	Procedures for preventing and responding to spills and cleanup, documentation and notification procedures
	
	

	Spill prevention and response – on-site responsibility
	A.17.e.i
	Indicate who is responsible for on-site management of significant materials and include their contact information
	
	

	Spill prevention and response – tenants
	A.17.e.i (1)
	If applicable, indicate how spill response will be coordinated between the permit registrant and otherwise unpermitted tenants
	
	

	Spill prevention and response – spills and leaks
	A.8.h.vi
	Procedures for expeditiously stopping, containing and cleaning up leaks, spills and other releases
	
	

	Spill prevention and response – state notification
	A.8.h.vii
	Procedures for immediate notification of appropriate facility personnel, DEQ or agent, and the Oregon Emergency Response System (1-800-452-0311),
when a spill may endanger health or the environment
	
	

	Spill prevention and response – local notification
	A.8.h.vii
	Include applicable requirements and contacts for reporting spills or unpermitted discharges to municipalities, local emergency services, public health and drinking water supply agencies
	
	

	Operations and maintenance – BMPs
	A.17.f
	Schedules or frequency of maintaining all control measures
	
	

	Operations and maintenance – treatment
	A.17.g
	Include, as appropriate to the type of treatment system, items such as system schematic, manufacturer’s
maintenance/operation specifications, chemical use, treatment volumes
	
	

	Operations and maintenance
	A.17.d.vii A.17.g
	Include operation and maintenance procedures related to source control, active, passive treatment and low impact
development control measures, such as mass reduction measures
	
	

	Operations and maintenance – SDS
	A.17.d.vii
	Include safety data sheets for any stormwater treatment chemicals or
substances used in stormwater treatment and stored on site
	
	

	Employee education
	A.8.j
	Develop and maintain an employee orientation and education program to inform personnel of the pertinent
components and goals of this permit and the SWPCP
	
	

	Employee education – frequency
	A.8.j.iii
(1)(2)
	Education training must occur no later than 30 calendar days of hire or change in duties, annually thereafter
	
	

	Employee education – frequency
	A.8.j.iii (3) A-D
	Education training must occur no later than 60 calendar days after revised SWPCP in response to:
· Operation or control measures that may significantly change the nature of pollutants present in stormwater discharge or significantly increase the pollutant(s) levels
· Discharge frequency
· Discharge volume or flow rate
· Monitoring location or discharge points
	
	

	Employee education
	A.17.h
	Include a description of the training content and the required frequency
	
	

	Tier 2 status
	A.17.d.vi
	Description of stormwater treatment controls or source controls, including low impact development, and implementation dates of approved Tier 2 corrective action response, including approved background waiver
	
	

	Discharge points
	A.d.x
	Identify each discharge point and the location(s) where stormwater monitoring will occur
	
	

	Discharge points – substantially similar
	A.d.x
	Existing discharge points excluded from monitoring must include a description of the discharge point(s) and data or analysis supporting that the discharge point(s) are substantially similar
	
	



Non-discrimination statement
DEQ does not discriminate on the basis of race, color, national origin, disability, age, sex, religion, sexual orientation, gender identity, or marital status in the administration of its programs and activities. For translations or alternate formats, visit DEQ’s Civil Rights and Environmental Justice page.
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